# Unit settings

### 1. Summary

Various settings can be specified for the unit.

### 2. Top page

This is the top page for unit settings. A description of each setting is shown.

#### 2.1. Unit name setting

Displays the unit name that is set.

- Press the "Setting" button to access a page where you can change the settings.

#### 2.2. LED mode setting

Displays the LED mode that is set.

- Press the "Setting" button to access a page where you can change the settings.

#### 2.3. Time zone setting

The time zone setting is shown.

- Press the "Setting" button to access a page where you can change the settings.

#### 2.4. Current date and time setting

The current date and time specified for this unit are shown.

- Press the "Setting" button to access a page where you can change the settings.

#### 2.5. Date and time synchronization setting

The NTP server that is queried at the specified time and date synchronization interval is shown.

- Press the "Next" button to access a page where you can synchronize the time.

- Press the "Setting" button to access a page where you can change the settings.

### 3. Unit name setting page

In this page you can set the unit name.

When you have entered the settings, press the "Confirm" button. If there are no mistakes in the input content confirmation screen, press the "OK" button.

#### 3.1. Unit name setting

- Unit name

  - Enter an arbitrary character string for use as the hostname.

  - Enter up to 63 single-byte alphanumeric characters or single-byte symbols.

### 4. LED mode setting page

In this page you can set the LED mode.

When you have entered the settings, press the "Confirm" button. If there are no mistakes in the input content confirmation screen, press the "OK" button.

#### 4.1. LED mode setting

- LED mode

  - Select the LED mode from the following.

    - LINK/ACT mode

      - LED indicator lights will illuminate, flash, or switch OFF depending on the LAN port status.

    - OFF mode

      - LED always stays off.

### 5. Time zone setting page

In this page you can set the time zone.

When you have entered the settings, press the "Confirm" button. If there are no mistakes in the input content confirmation screen, press the "OK" button.

#### 5.1. Time zone setting

- Time zone

  - Select the time zone from the following.

    - UTC

    - JST

    - Difference from GMT ( -12:00 to +13:00 )

### 6. Current date and time setting page

In this page you can set the current date and time.

When you have entered the settings, press the "Confirm" button. If there are no mistakes in the input content confirmation screen, press the "OK" button.

#### 6.1. Current date and time setting

- Current time

  - In the "year/month/date" box, enter the date in YYYY/MM/DD format.

    - When you move the focus to the box, a calender is displayed. You can select a date to enter that date in the box.

    - You can also enter this manually.

  - In the "hours:minutes:seconds" box, enter the time in hh:mm:ss format.

    - When you move the focus to the box, a calender is displayed. You can select a date to enter that date in the box.

    - You can also enter this manually.

### 7. Date and time synchronization page

In this page you can synchronize the time with an NTP server.

When you press the "OK" button, the time is synchronized with the NTP server that is specified as the query destination.

### 8. Date and time synchronization setting page

In this page you can make settings for synchronization with an NTP server.

When you have entered the settings, press the "Confirm" button. If there are no mistakes in the input content confirmation screen, press the "OK" button.

#### 8.1. Date and time synchronization setting

- Date and time synchronization interval

  - Specifies the interval at which time is synchronized with the NTP server.

  - You can choose from the following as the synchronization interval.

    - Unused

    - 1 hour — 24 hours

  - Periodic time synchronization is disabled by default.

- NTP server to query

  - Enter the host name or IP address of the NTP server that will perform synchronization.

  - Up to two NTP servers can be configured.

Search result
No more search results.
There are no topics that match your search query.