# CONFIG management

### 1. Summary

In this page you can import and export CONFIG files.

This unit operates in accordance with its CONFIG file (settings data). A CONFIG file consists of a combination of multiple commands.

### 2. Top page

This is the top page for CONFIG file management.

Here you can start the process of importing a CONFIG file from the PC, or the process of exporting a CONFIG file to the PC.

#### 2.1. Import CONFIG file

- Press the "Next" button to begin the process of importing a CONFIG file from the PC.

#### 2.2. Export CONFIG file

- Press the "Next" button to begin the process of exporting a CONFIG file to the PC.

### 3. Import CONFIG file page

In this page, a CONFIG file from the PC can be copied to internal non-volatile memory, updating the CONFIG file.

When you have entered the settings, press the "Confirm" button. If there are no mistakes in the input content confirmation screen, press the "OK" button.

If the currently used CONFIG file is the same as the import-destination CONFIG file, the unit restarts automatically after the import has ended successfully.

#### 3.1. Import CONFIG file

- Currently-used CONFIG file

  - The currently used CONFIG file is shown.

- File to import

  - Press the "Select a file" button to display the file selection dialog box.

- Import-destination file

  - Select the import-destination CONFIG file in internal non-volatile memory.

### 4. Export CONFIG file page

In this page you can copy a CONFIG file from internal non-volatile memory to the PC.

When you have finished entry, check the entered content and press the "OK" button.

#### 4.1. Export CONFIG file

- Currently-used CONFIG file

  - The currently used CONFIG file is shown.

- File to export

  - Select the CONFIG file in internal non-volatile memory that you want to export.

Search result
No more search results.
There are no topics that match your search query.