# Various server settings

### 1. Summary

In this page you can make settings for each type of server.

### 2. Top page

This is the top page for making settings for each type of server.
The current settings are shown for the servers listed below.

- HTTP server

- Telnet server

- TFTP server

- SNMP server

#### 2.1. Web GUI access

- Displays the settings for the HTTP server.

- The table items are explained below.

  - Port number of HTTP server

    - Displays the port number of HTTP server.

  - Use secure HTTP server

    - Displays whether a secure HTTP server is to be used or not.

    - If a secure HTTP server is to be used, the port number will be displayed.

  - Clients that can access the HTTP server

    - Displays the clients that can access the HTTP server.

  - Time until auto logout

    - Displays the time until auto logout.

#### 2.2. Access via Telnet

- Displays the settings for the Telnet server.

- The table items are explained below.

  - Use Telnet server

    - Displays whether a Telnet server is to be used or not.

    - If a Telnet server is to be used, the port number will be displayed.

  - Clients that can access the Telnet server

    - Displays the clients that can access the Telnet server.

#### 2.3. Access via TFTP

- Displays the settings for the TFTP server.

- The table items are explained below.

  - Use TFTP server

    - Displays whether a TFTP server is to be used or not.

    - If a TFTP server is to be used, the port number will be displayed.

  - Clients that can access the TFTP server

    - Displays the clients that can access the TFTP server.

#### 2.4. Access via SNMP

- Displays the settings for the SNMP server

- The table items are explained below.

  - Clients that can access the SNMP server

    - Displays the clients that can access the SNMP server.

### 3. Web GUI access settings page

In this page you can configure the settings for an HTTP server.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 3.1. Web GUI access

- Port number of HTTP server

  - Specifies the port number of HTTP server.

  - Input a port number from 1 to 65535.

- Use secure HTTP server

  - Select below whether an secure HTTP server will be used or not.

    - Use

    - Don’t use

  - When Use is selected, specify the port number.

  - Input a port number from 1 to 65535.

- Clients that can access the HTTP server

  - Select the client access restriction methods from the following options.

    - Permit all

    - Specify conditions

  - When Specify conditions is selected, up to 8 conditions can be specified.

  - The conditions are specified as shown below.

    - Operation

      - To restrict client access, select from the following operations.

        - Permit

        - Deny

    - Conditional

      - Select from the following targets for client access restriction.

        - All addresses

        - Specified IP address

    - IP address

      - When Specified IP address is selected, specify the IP address.

      - The following IP addresses shown below can be specified.

        - IPv4 address

          - Example: 192.168.100.1

        - IPv4 network address

          - Example: 192.168.100.0/24

        - IPv6 address

          - Example: fe80::1234:5678

        - IPv6 network address

          - Example: 2001:1234:5678:90ab::0/64

  - Conditions are evaluated in ascending order of numbers.

  - If even one condition is specified, all access from clients that do not meet any condition will be denied.

  - Press the icon to add a configuration form.

  - Press the "Delete" button to delete a configuration form.

- Time until auto logout

  - In the list box, select the time until auto logout.

  - If the desired time setting is not shown in the list box, select "Specify" and enter the desired time setting in the text box below the list box.

  - Any time setting within the range of 1 - 120 minutes may be entered.

### 4. Access via Telnet settings page

In this page you can configure the settings for a Telnet server.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 4.1. Access via Telnet

- Use Telnet server

  - Select below whether a Telnet server will be used or not.

    - Use

    - Don’t use

  - When Use is selected, specify the port number.

  - Input a port number from 1 to 65535.

- Clients that can access the Telnet server

  - The setting method for this item is the same as for the "Clients that can access the HTTP server" item on the Web GUI access page.

### 5. Access via TFTP settings page

In this page you can configure the settings for a TFTP server.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 5.1. Access via TFTP

- Use TFTP server

  - Select below whether a TFTP server will be used or not.

    - Use

    - Don’t use

  - When Use is selected, specify the port number.

  - Input a port number from 1 to 65535.

- Clients that can access the TFTP server

  - The setting method for this item is the same as for the "Clients that can access the HTTP server" item on the Web GUI access page.

### 6. Access via SNMP settings page

Displays the settings for the SNMP server.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 6.1. Access via SNMP

- Clients that can access the SNMP server

  - Select the client access restriction methods from the following options.

    - Permit all

    - Specify access conditions

  - When Specify conditions is selected, up to 32 conditions can be specified.

- Access condition

  - Specify condition for to restrict access from client.

  - Press the or icons to change the order in which the access conditions are applied.

  - Following points about SNMP server access condition differ from other type servers.

    - Access restriction behavior is always "Permit".

    - Community or user that apply condition can be selected.

  - The setting method for other item is the same as for the "Clients that can access the HTTP server" item on the Web GUI access page.

Search result
No more search results.
There are no topics that match your search query.