# Create Access list

### 1. Summary

In this page you can create or delete access lists, and change their settings.

### 2. Top page

This is the top page for creating an access list.

#### 2.1. Access lists

- The information for the access list you created will be displayed.

- The table items are explained below.

  - ID

    - The access list ID will be displayed.

  - Type

    - The access list type will be displayed.

  - Comment

    - The comment set in this access list will be displayed.

- A maximum of 20 items can be displayed for one page. Press or or enter a numeric value to switch between pages.

- You can press the sort switch to sort by each item.

- Press the "New" button to display the page where you can create a new access list.

- Press the "Setting" button to show the page where you can change the settings of the selected access list.

- If you press the "Delete" button, all access lists whose check boxes are selected will be deleted.

- On this page, you can reference and configure up to 28 access list for each access list type of IPv4/IPv6/MAC.

### 3. Access list settings page

This page is for creating new access lists, or for changing the settings of existing access lists.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 3.1. Access list settings

- Access list

  - Select the access list type from the following items.

    - IPv4 access list

    - IPv6 access list

    - MAC access list

  - When changing the settings, the access list type cannot be changed.

- Access list ID

  - Set the configurable access list ID from the following ranges, according to the access list type.

    - IPv4 access lists

      - 1 - 2000

    - IPv6 access lists

      - 3001 - 4000

    - MAC access lists

      - 2001 - 3000

  - When changing the settings, the access list ID cannot be changed.

- Comment

  - Specify the comment using up to 32 single-byte alphanumeric characters and symbols.

  - The "?" character cannot be used in the comment text.

- Control conditions

  - Specify the control conditions for the access list.

  - Up to 128 control conditions can be configured per access list.

  - Press the "Add" button to display the "Control condition settings" dialog.

  - In the "Control condition settings" dialog, you can specify conditions for which traffic is permitted and denied as per the following items.

    - Operation

      - Select the actions to be taken when the traffic matches the control conditions, shown in the items below.

        - Permit

        - Deny

    - Source address

      - Select the source address to be targeted from the following items.

        - All addresses

        - Specify host address

        - Specifying a network address

          - This cannot be specified for a MAC access list.

        - Specify host address with wildcard bit

          - Specify the address and wildcard mask.

          - This cannot be specified for a IPv6 access list.

      - If the wildcard mask bit is "1," the bit in the same address position will not be checked.

      - When specifying the conditions for subnet 192.168.1.0/24, do so as shown below.

        - Address : 192.168.1.0, Wildcard mask : 0.0.0.255

      - When specifying the conditions for vendor code 00-A0-DE---*, do so as shown below.

        - Address : 00A0.DE00.0000, Wildcard mask : 0000.00FF.FFFF

  - Press the "Delete" button to delete the corresponding control conditions.

  - Press the or icons to change the order in which the control conditions are applied.

  - When evaluating the control conditions, control conditions with earlier numbers will be evaluated first; and if the conditions match, the conditions that follow will not be checked.

Search result
No more search results.
There are no topics that match your search query.