# Physical interface

### 1. Summary

This page is for changing the physical interface settings.

### 2. Top page

This is the top page for the physical interface settings.

#### 2.1. MRU setting

- The MRU settings is shown.

- The table items are explained below.

  - MRU

    - Displays the maximum amount of data that can be received at one time.

- Press the “Setting” button to show the MRU settings page.

#### 2.2. Interface list

- The current operating status and settings for the physical interface are shown for each interface.

- The table items are explained below.

  - Check box

    - Select the check box for bulk settings or to initialize the settings.

  - Port

    - Displays the interface name.

  - Link

    - Displays the link status for the interface.

  - Speed/communication mode

    - Displays the operating speed and communication mode.

    - For automatic settings, “(Automatic)” is displayed at the end of the status indication.

  - EEE function

    - Displays the operating status of the EEE function.

  - Automatic cross/straight detection

    - Displays the operating status of the automatic cross/straight detection.

  - Explanation

    - Displays the description text that is set for the interface.

- Press the "Setting" button to display the page where you can change the settings of the selected interface.

- If you press the "Specify all" button, the settings can be changed for all interfaces whose check box is selected.

  - The default settings will be applied to the settings on the physical interface settings page.

- If you press the "Return to defaults" button, the settings will be initialized on all interfaces whose check boxes are selected.

  - Each of the default settings are shown below.

    - Operation : Enable interface

    - Explanation : Unset

    - Speed/communication mode : Automatic

    - EEE function : Disabled (Don’t use power-conservation Ethernet function)

    - Automatic cross/straight detection : Enabled

### 3. MRU settings page

This page is for configuring the MRU settings.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 3.1. MRU setting

- MRU

  - Specify the maximum amount of data that can be received at one time.

  - The input range is 1522 - 10240 bytes.

### 4. Physical interface settings page

This page is for changing physical interface-related settings.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 4.1. Physical interface settings

- Port

  - Displays the name of the interface for which settings will be made.

- Operation

  - Select from the following interface operations.

    - Enable interface

    - Disable interface

- Explanation

  - Sets the interface description text.

  - Characters that can be inputted include single-byte alphanumeric characters and symbols, excluding ?.

  - Up to 80 characters can be inputted.

- Speed/communication mode

  - Select the interface speed and communication method from the following options.

    - For a LAN port

      - Automatic

      - 1Gbps / Full duplex

      - 100Mbps / Full duplex

      - 100Mbps / Half duplex

      - 10Mbps / Full duplex

      - 10Mbps / Half duplex

- EEE function

  - Select the operation for the EEE function from the following options.

    - Disabled (Don’t use power-conservation Ethernet function)

    - Enabled (Use power-conservation Ethernet function)

- Automatic cross/straight detection

  - Select the operation for the automatic cross/straight detection from the following options.

    - Enabled

    - Disabled

  - If the automatic cross/straight detection is disabled, MDI is used for the cable connection type.

Search result
No more search results.
There are no topics that match your search query.