# List of Default Settings

SWX2210P series default settings are indicated below.

- System-wide default settings

  Category | Setting Parameter | Setting value
  --- | --- | ---
  Console | Telnet console timeout | 600 sec
  Number of VTYs | 4
  Number of lines displayed | 24
  Password | Default administrative user | User name: admin Password: admin
  Administrator password | admin
  Encrypt password | Not encrypted
  Time Management | Time zone | JST (UTC＋9.0)
  NTP server | None
  NTP update cycle | None
  SNMP | Action | Disabled
  SYSLOG | debug level log output | OFF
  information level log output | ON
  error level log output | ON
  SYSLOG server | None
  Firmware Update | Download URL | For SWX2210P-10G: firmware-update url http://www.rtpro.yamaha.co.jp/firmware/revision-up/swx2210p-10g.bin For SWX2210P-18G: firmware-update url http://www.rtpro.yamaha.co.jp/firmware/revision-up/swx2210p-18g.bin For SWX2210P-28G: firmware-update url http://www.rtpro.yamaha.co.jp/firmware/revision-up/swx2210p-28g.bin
  Permit downward revision | Prohibit
  Timeout | 300 sec
  LLDP | Action | Enabled
  Automatic setting function | Enabled
  L2MS | Action | Enabled
  Role | Agent
  Access control | Telnet server status | Start (port 23)
  Telnet server access | Allow access from all hosts
  TFTP server status | Do not start
  HTTP server status | Start (port 80)
  Secure HTTP server status | Start (port 443)
  HTTP/HTTPS server access | Allow access from all hosts
  SNMP server status | Start (port 161)
  SNMP server access | Allow access from all hosts
  Interface control | MRU | 1,522 Byte
  BPDU pass through | Enabled
  EAP pass through | Enabled
  Link Aggregation | None
  L2 switching | Automatic MAC address acquisition | Enabled
  Automatic MAC address acquisition aging time | 300 sec
  Proprietary Loop Detection | Enabled
  Multiple VLAN | None
  IP multicast | IGMP snooping | Disabled
  MLD snooping | Disabled
  DNS client | Action | Enabled
  Traffic control | QoS | Disabled
  Flow control (IEEE 802.3x) | Disabled
  PoE supply | Power supply actions | Enabled
  Guard band | 7 W
  Web GUI | Language setting | Japanese

- Default settings per LAN port

  Category | Setting Parameter | Setting value
  --- | --- | ---
  Basic settings | Speed/communication mode setting | auto
  Cross/straight automatic detection | Enabled
  Port description | None
  EEE | Disabled
  Port Mode | Access
  Associated VLAN ID | 1 (default VLAN)
  L2MS | L2MS filter | Disabled
  non-L2MS filter | Disabled
  L2 switching | Proprietary Loop Detection | Enabled
  Traffic control | QoS trust mode | CoS
  Flow control (IEEE 802.3x) | Disabled
  Storm Control | Disabled
  LLDP agent | Transmit/receive mode | Enabled
  PoE supply | Power supply actions | Enabled
  PoE power priority | Low

- Settings for default VLAN (vlan1)

  Setting Parameter | Setting value
  --- | ---
  IPv4 Address | 192.168.100.240/24
  IGMP Snooping | Action | Disabled
  MLD Snooping | Action | Disabled

Search result
No more search results.
There are no topics that match your search query.