# SYSLOG management

### 1. Summary

In this page you can view and edit the settings of the SYSLOG function.

The operation history of this device is output as the SYSLOG (log data) according to the settings of the SYSLOG function. In addition to recording the SYSLOG inside this device, you can also specify a destination address for output to an external host.

### 2. Top page

This is the top page for SYSLOG management.

The current settings for the SYSLOG function are shown.

#### 2.1. SYSLOG settings

- The type of SYSLOG that is output, and the header information and destination address for the SYSLOG transmission are shown.

- Press the "Setting" button to access a page where you can change the settings.

### 3. SYSLOG settings page

In this page you can make settings for the SYSLOG function.

When you have entered the settings, press the "Confirm" button. If there are no mistakes in the input content confirmation screen, press the "OK" button.

For details on the various SYSLOG types, refer to the command reference.

#### 3.1. SYSLOG settings

- SYSLOG type

  - DEBUG

    - This setting specifies whether DEBUG type SYSLOG is output.

  - INFO

    - This setting specifies whether INFO type SYSLOG is output.

  - ERROR

    - This setting specifies whether ERROR type SYSLOG is output.

- SYSLOG transmission

  - Header

    - This is the header setting when outputting the SYSLOG to an external host.

    - You can specify whether or not to include the time stamp and device name in the header of the SYSLOG message.

  - Destination address

    - This is the transmission destination address setting when outputting the SYSLOG to an external host.

    - You can specify up to two IPv4/IPv6 destination addresses.

    - For IPv6 link local addresses, you must also specify the interface to send from. (Format: fe80::X%vlanN)

    - If no destination address is specified, the SYSLOG is recorded only inside the switch.

Search result
No more search results.
There are no topics that match your search query.