# Update firmware

### 1. Summary

In this page you can perform operations related to firmware update.

### 2. Top page

This is the top page for firmware update.

You can start the procedure for updating the firmware via the network. Various settings for updating the firmware via the network are displayed.

#### 2.1. Current firmware revision

- The currently-used firmware revision is shown.

#### 2.2. Update firmware from PC

- When you press the "Next" button, the procedure for updating the firmware from the PC will be started.

#### 2.3. Update firmware via network

- When you press the "Next" button, the procedure for updating the firmware via the network will be started.

- Various settings for updating the firmware via the network are displayed.

- Press the "Setting" button to access a page where you can change the settings.

### 3. Update firmware from PC page

In this page you can specify the firmware file placed on the PC from which you are accessing the web GUI, and perform the firmware update.

In "Select file," select the firmware file that you want to use for the update, and press the "Confirm" button. If there are no mistakes in the confirmation screen, press the "OK" button.

Note that the unit will automatically restart when the firmware has been updated successfully.

#### 3.1. Update firmware from PC

- Specify update file

  - Selects the firmware file used for the update

### 4. Update firmware via network page

In this page you can download a firmware file from a web server, and perform the firmware update. This function lets you easily perform the entire process of checking for the latest firmware, downloading it, and updating the firmware.

When you open the page, the revision of the firmware file on the web server is automatically checked.

If the download URL is the Yamaha website and an updateable firmware revision is found. The "OK" button displays a guide to the software license agreement website. Please read the contents on the website and press the "OK" button if you agree to the terms. Press the "OK" button to start downloading the firmware file from the webserver.

Note that the unit will automatically restart when the firmware has been updated successfully.

#### 4.1. Update firmware via network

- Current firmware revision

  - The revision of the currently-used firmware file is shown.

- Firmware revision available for update

  - Updatable revisions of the firmware files on the web server are shown.

### 5. Firmware update basic settings page

In this page you can make various settings for updating the firmware via the network.

When you have entered the settings, press the "Confirm" button. If there are no mistakes in the input content confirmation screen, press the "OK" button.

#### 5.1. Firmware update basic settings

- Download source URL

  - This is the setting of the URL at which the firmware is located.

- HTTP proxy server

  - FQDN or IP address

    - Specify a proxy server FQDN or IP address that is no more than 255 single-byte alphanumeric or symbol characters long.

  - Port number

    - Specifies the port number of the proxy server.

    - Input a port number from 1 to 65535.

- HTTPS proxy server

  - FQDN or IP address

    - Specify a proxy server FQDN or IP address that is no more than 255 single-byte alphanumeric or symbol characters long.

  - Port number

    - Specifies the port number of the proxy server.

    - Input a port number from 1 to 65535.

- Revision downgrade

  - This setting permits or forbids rewriting to an older version of firmware.

- Timeout

  - This setting specifies the timeout time during the process of updating the firmware via the network.

Search result
No more search results.
There are no topics that match your search query.