# Pass through

### 1. Summary

In this page you can edit the settings of the pass through function.
You can enable/disable the pass through function.

### 2. Top page

This is the top page for pass through.

#### 2.1. EAP pass through setting

- The current setting is shown as to whether the EAP pass through is enabled.

- EAP frames are used for IEEE 802.1X authentication.

- If EAP pass through is enabled, the unit can be installed between an IEEE 802.1X authentication switch and a computer.

- Press the "Setting" button to access a page where you can change the settings.

#### 2.2. BPDU pass through setting

- The current setting is shown as to whether the BPDU pass through is enabled.

- BPDU frames are used in the spanning tree protocol (STP).

- If BPDU pass through is enabled, the unit can be installed between switches using STP.

- Press the "Setting" button to access a page where you can change the settings.

### 3. EAP pass through settings page

In this page you can specify whether the EAP pass through is enabled.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 3.1. EAP pass through setting

- EAP pass through

  - Enabled

    - Forwards received EAP frames.

  - Disabled

    - Discards received EAP frames.

### 4. BPDU pass through settings page

In this page you can specify whether the BPDU pass through is enabled.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 4.1. BPDU pass through setting

- BPDU pass through

  - Enabled

    - Forwards received BPDU frames.

  - Disabled

    - Discards received BPDU frames.

Search result
No more search results.
There are no topics that match your search query.