# Link aggregation

### 1. Summary

This page is for configuring the link aggregation settings.

### 2. Top page

This is the top page for the link aggregation.

#### 2.1. Load balance rule settings

- Shows the load balance rule settings.

- The table items are explained below.

  - Load balance rule

    - Displays the load balance rule settings.

- Press the “Setting” button to show the page for the load balance rule settings.

#### 2.2. Interface list

- The operating status and settings are shown for the logical interface and the physical interface.

- The table items are explained below.

  - Check box

    - Select the check box to delete the logical interface.

  - Port

    - Displays the interface name.

  - Link

    - Displays the link status for the interface.

  - Explanation

    - Displays the description text that is set for the interface.

- Press the "New" button to display a page where you can create new settings for a logical interface.

- Press the "Setting" button to display the page where you can change the settings of the selected logical interface.

- If you press the "Delete" button, all logical interfaces whose check boxes are selected will be deleted.

  - When deleting a logical interface, you can specify the physical interface operations after deletion as follows.

    - Enable

    - Disable

- Up to 8 logical interfaces can be configured.

### 3. Load balance rule settings page

This page is for configuring the load balance rule settings.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 3.1. Load balance rule settings

- Load balance rule

  - The following load balance rules can be selected.

    - Destination MAC address

    - Source MAC address

    - Destination/source MAC address

    - Destination IP address

    - Source IP address

    - Destination/source IP address

    - Destination port number

    - Source port number

    - Destination/source port numbers

### 4. Logical interface settings page

This page is for changing the logical interface settings.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 4.1. Logical interface settings

- Logical interface type

  - When configuring new settings

    - Displays the type of logical interface.

  - When changing settings

    - Displays the selected logical interface name.

- Interface number

  - Specifies the interface number.

  - A value from 1 to 8 can be inputted.

  - This item will be displayed only when configuring new settings.

- Associated port

  - Select the port that will be associated with the logical interface.

  - Press the "Select" button to display the “Physical interface list” dialog box.

  - Select the port check box in the “Physical interface list” dialog box and press the “OK” button to select the associated port.

  - Up to 8 ports can be selected.

- Operation

  - Select from the following logical interface operations.

    - Enable interface

    - Disable interface

- Explanation

  - Sets the interface description text.

  - Characters that can be inputted include single-byte alphanumeric characters and symbols, excluding ?.

  - Up to 80 characters can be inputted.

Search result
No more search results.
There are no topics that match your search query.