# About each screen

### 1. Dashboard

It shows the various system information of this device in visual form. You can check and monitor the following status.

- Interface information

- System information

- Resource information ( CPU Utilization / MemoryUtilization )

- SYSLOG

- Traffic information ( Transmit / Reception )

- Resource information ( Graph )

### 2. ProAV settings

In this page you can make ProAV settings for this unit. The following items are provided.

- ProAV profile

- Multicast

### 3. Detailed settings

In this page you can make detailed network-related settings for this unit. The following items are provided.

- Basic settings

- Interface settings

  - Physical interface

  - Port mirroring

  - Link aggregation

  - PoE control

- VLAN

  - Create VLAN

  - Tag VLAN

  - Multiple VLAN

- Layer 2 functions

  - MAC address table

  - Loop detected

  - Pass through

- Layer 3 functions

  - DNS client

- Multicast

  - Multicast basic settings

  - IGMP snooping

  - MLD snooping

- Traffic control

  - Access list

    - Create Access list

    - Apply Access list

  - QoS

  - Flow control

  - Storm control

### 4. Management

In this page you can make settings for this unit, and perform maintenance. The following items are provided.

- Unit settings

- Access management

  - User settings

  - Various server settings

- Schedule execution

- SNMP

  - MIB

  - Community

  - SNMPv3 User

  - SNMP trap

- LLDP

- L2MS

- Maintenance

  - Command execution

  - Update firmware

  - CONFIG management

  - SYSLOG management

  - Restart and initialization

  - Cable diagnostics

### 5. CONFIG

The results of running the "show running-config" command (a setting of this unit) can be viewed in a web browser or acquired as a text file.

- Viewing CONFIG

  - In the "CONFIG" menu, press the "Show in browser" button. The execution result of the "show running-config" command is shown in a sub-window.

  - To close, press the web browser’s close button.

- Obtaining CONFIG as a text file

  - In the "CONFIG" menu, press the "Obtain as text file" button to start the download automatically.

  - The name of the acquired file is "running-config_YYYYMMDDhhmmss.txt".

    YYYY | …​ | A.D. ( 4 Digit )
    MM | …​ | Month ( 2 Digit )
    DD | …​ | Day ( 2 Digit )
    hh | …​ | Hours ( 2 Digit )
    mm | …​ | Minutes ( 2 Digit )
    ss | …​ | Seconds ( 2 Digit )

### 6. SYSLOG

This feature outputs the log of this unit’s operation status in the order of the oldest occurrence time.
In the "SYSLOG" menu, the result of running the show logging command can be viewed in a web browser or acquired as a text file.

- Viewing SYSLOG

  - In the "SYSLOG" menu, press the "Show in browser" button. The execution result of the "show logging" command is shown in a sub-window.

  - To close, press the web browser’s close button.

- Obtaining SYSLOG as a text file

  - In the "SYSLOG" menu, press the "Obtain as text file" button to start the download automatically.

  - The name of the acquired file is "running-config_YYYYMMDDhhmmss.txt".

    YYYY | …​ | A.D. ( 4 Digit )
    MM | …​ | Month ( 2 Digit )
    DD | …​ | Day ( 2 Digit )
    hh | …​ | Hours ( 2 Digit )
    mm | …​ | Minutes ( 2 Digit )
    ss | …​ | Seconds ( 2 Digit )

### 7. TECHINFO

The "show tech-support" command lets you view status information for all of this unit’s functions.
In the "TECHINFO" menu, the results of running the "show tech-support" command can be viewed in a web browser or acquired as a text file.

- Viewing TECHNIFO

  - In the "TECHINFO" menu, press the "Show in browser" button. The execution result of the "show tech-support" command is shown.

  - To close, press the web browser’s close button.

- Obtaining TECHNIFO as a text file

  - In the "TECHINFO" menu, press the "Obtain as text file" button to start the download automatically.

  - The name of the acquired file is "technifo_YYYYMMDDhhmmss.txt".

    YYYY | …​ | A.D. ( 4 Digit )
    MM | …​ | Month ( 2 Digit )
    DD | …​ | Day ( 2 Digit )
    hh | …​ | Hours ( 2 Digit )
    mm | …​ | Minutes ( 2 Digit )
    ss | …​ | Seconds ( 2 Digit )

- Notes

  - It may take some time to obtain TECHNIFO.

  - This unit may undergo loading while the information is being acquired.

Search result
No more search results.
There are no topics that match your search query.