# Schedule execution

### 1. Summary

In this page you can make settings for schedule execution.

The schedule execution function of this product has two setting items, schedule template and schedule.

Schedule template settings allow you to create a template of detailed settings for processes involved in executing scheduled functions and operations, such as the specific functions to be executed, the applicable item involved, and the execution sequence.

In schedule settings, you can select when to execute schedules and which templates to execute.

### 2. Top page

This is the top page for making settings for schedule execution.

#### 2.1. List of schedule template

- Information for the currently registered schedule template are shown.

- The table items are explained below.

  - Template ID

    - Registered schedule template ID are shown.

  - Status

    - The status of the schedule template are shown.

  - Template description

    - Description of the schedule template are shown.

- If you press the "New" button, a page appears in which you can create a new schedule template.

- If you press the "Setting" button, a page appears in which you can edit the settings of the selected schedule template.

- If you press the "Delete" button, all schedule templates whose check box has a check mark will be deleted.

- Up to 10 schedule templates can be registered.

#### 2.2. List of schedule

- Information for the currently registered schedule are shown.

- The table items are explained below.

  - Schedule ID

    - Registered schedule ID are shown.

  - Execution timing

    - The execution timing of the schedule are shown.

  - Template to be executed

    - The information about the template to be executed when the schedule executed are shown.

- If you press the "New" button, a page appears in which you can create a new schedule.

- If you press the "Setting" button, a page appears in which you can edit the settings of the selected schedule.

- If you press the "Delete" button, all schedules whose check box has a check mark will be deleted.

- Up to 10 schedules can be registered.

### 3. Schedule template settings page

In this page you can create a new schedule template or edit the settings of an already-registered schedule template.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 3.1. Schedule template settings

- Template ID

  - The ID of the schedule template being set is displayed.

  - Newly created templates are automatically assigned the lowest unregistered serial number as the template ID.

- Template description

  - Sets the schedule template description text.

  - Characters that can be inputted include single-byte alphanumeric characters and symbols, excluding ?.

  - Up to 64 characters can be inputted.

- Template status

  - Select template status from the following items.

    - Enabled

      - Enables the template

    - Disabled

      - Disables the template

- Contents of schedule execution

  - Specify the following items as the schedule execution contents.

    - Function to be executed

      - Select the function to be executed by schedule execution from the following items.

        - Shutdown

        - Cancel shutdown

        - Disable PoE power supply

        - Enable PoE power supply

        - Save settings

    - Applicable item

      - Select the applicable item of the function to be executed.

      - The choices available for the applicable item setting vary depending on the settings selected in the "Function to be executed" field.

  - "Execution cost" is the cost required for storing scheduled processes for execution inside the product and corresponds to the number of cli-command lines.

  - This product allows using an execution cost up to 100 for each template.

  - Specify settings so that the total "execution cost" is 100 or less.

  - Click the icon to add a configuration form.

  - Click the “Delete” button to delete a configuration form.

  - Execution content specified or edited outside the schedule template settings screen is displayed in command format.

  - If editing a template displayed in command format, enter the setting in console command format (abbreviated input is not accepted).

  - You can enter multiple commands together by separating them with line-returns.

  - Specify settings that result in 100 or fewer command lines.

  - Schedule execution always starts with the specially-privileged EXEC mode (enable).

  - The commands that can be set are as follows.

    - configure terminal

    - interface

    - shutdown

    - no shutdown

    - power-inline disable

    - power-inline enable

    - write

    - end

    - exit (Cannot be executed in "special privilege EXEC mode")

  - For details on commands to enter, refer to the command reference and to the information provided on the Network device product information page and Network device technical information page.

### 4. Schedule settings page

In this page you can create a new schedule or edit the settings of an already-registered schedule.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 4.1. Schedule settings

- Schedule ID

  - The ID of the schedule being set is displayed.

  - Newly created templates are automatically assigned the lowest unregistered serial number as the schedule ID.

- Execution timing

  - Select the timing to execute the schedule execution.

    - Easy input

      - Select a typical frequency pattern for the schedule execution timing.

      - Period

        - Select the periodic pattern of schedule execution from the following items.

          - Every day

          - Every week

          - Every month

          - Every year

        - If "Every week" is selected, mark the checkbox for the day of the week when the schedule is to be executed.

        - If "Every month" is selected, enter the day when the schedule is to be executed in the "Day" box.

        - If "Every year" is selected, enter the month and the day when the schedule is to be executed in the "Month" box and the "Day" box.

        - Enter numeric values in the "Month" and "Day" boxes.

        - Multiple months/days can be specified as comma-delimited values. (Example: Enter "10,20" to specify 10 and 20.)

        - A hyphen can be used to indicate a range of values. (Example: Enter "1-3" to specify 1, 2, and 3.)

        - When you focus on the "Month" and "Day" boxes, the input form that can be operated with a mouse click is displayed.

      - Time

        - In the "hours:minutes:seconds" box, enter the time in hh:mm:ss format.

        - When you focus on the "Hour:Minute:Second" box, an input form that can be operated with a mouse click is displayed.

    - Input in command format

      - Enter the "Date" and "Time" in the command format.

      - This allows specifying settings in more detail than the Easy input mode.

      - Enter the date in MONTH/DATE format.

      - Enter the time in the hh:mm:ss format.

      - For details on command format, refer to the command reference and to the information provided on the Network device product information page and Network device technical information page.

- Template to be executed

  - Select the template to be executed in the schedule execution.

Search result
No more search results.
There are no topics that match your search query.